Product specification

|  |  |
| --- | --- |
| Voltage supply | 5 V |
| Typical operating current | 470 mA |
| Dimensions | 131x69x44 |
| Operational Temperature | 16°C to 26°C |
| Humidity range | 15%RH to 65%RH |
| Output/Concentration Resolution | 1ppm |
| Temperature resolution | 1°C |
| Humidity resolution | 1%RH |
| Weight | ? |
| Max. distance between receiver and transmitter | 26 m(open space) |
| Logging speed | 2 seconds |
| Bandwidth | ? |